Changes from 1.3.129TViX HD M-6500 1.3.147/1.3.148(UJuckbox) Release note

  audio playlist Manual 

 

1)      Added the Audio playlist function (* Please download the detailed guide for the audio playlist function)

-          Select multiple songs that you want to listen and save them as a playlist conveniently (to be saved in Audio/Playlist folder)

-          When pressing ¡®Audio¡¯ key on the remote, it will move to the Audio/Playlist folder automatically

-          Listen to music without TV or display

¡¤         When setting Autorun in setup, the first playlist in the Audio/Playlist folder will be played automatically unless there is  ¡°autorun¡± folder.

 

2)       Contents native resolution output function has been Added

(Please read below carefully before use the ¡°Native resolution¡± feature. If a user do not set resolution correctly, the video may not be displayed or I might hurt display. Please use this function with caution )

 

2-1) Native Resolution menu on ¡°SET UP¡± 

-          If a user turns on Native Resolution on the Setup-Video/Audio, the Auto NTSC/PAL/24Hz option will be disabled and will not be used. The NTSC/PAL/24Hz option will be functional if and only if Native Resolution is turned off.

-          When a user turns on Native Resolution, a popup, will be shown.

the user can select native content resolution output he want

¡¤         Users can turn on and off for the each resolution. 

¡¤         If the user turns on, the check box will be checked and when a video file is played, the source will be output according to the resolution and scan type(progressive/interlace) regardless of the current TV out setting.

¡¤         If the user turns off, the source will be scaled to the resolution and refresh rate set by the TV out setting in SET UP menu.

¡¤         If the user¡¯s display device does not support specific input mode, users will not see any video. In this case, just press stop and the video output mode will go back to the initial mode on  the SET UP menu..

¡¤         For the 720p, we separated the mode to ¡°720p24Hz¡± and ¡°1080p24Hz¡±, since most display devices do not support 720p24Hz mode. If users¡¯ displays do not support neither 720p24Hz nor 1080p24Hz, users will not be able to see 24Hz video clips.

 

2-2) Resolution change popup

-          If TVIX does not detect resolution and frame rate correctly, the Native Resolution will not work properly. In this case, users can press TV Out button while video clips are played. They can change to a specific output mode by selecting correct resolution and frame rate.

-          TV out button will show the Resolution change popup if the video clip is playing. Otherwise, it will change the Video mode NTSC->480p(DVI)->PAL->576p(DVI) for the a emergency recovery.(If a user use HDMI, a user must reset set video output mode on the using SETUP menu, otherwise, audio will not be sent over HDMI)

 

Available frame rate(refresh rate) table for each resolution 

 

480i
 59.94Hz, 60Hz
 
576i
 50Hz
 
480p
 59.94Hz, 60Hz
 
576p
 50Hz
 
720p
 23.976Hz, 24Hz, 29.97Hz, 30Hz, 50Hz, 59.94Hz, 60Hz
 
1080i
 50Hz, 59.94Hz, 60Hz
 
1080p
 23.976Hz, 24Hz, 29.97Hz, 30Hz, 50Hz, 59.94Hz, 60Hz
 


 

3)      Audio play besides audio playlist function

-          Fixed the shuffle function for autorun in setup

-          Supports M4A extension

 

4)      Video playing

-          Provides page up/down function with ¡®|<<¡¯, ¡®>>|¡¯ keys on the remote for the audio/subtitle/chapter pop-up

-          Rebooting problem when playing mkv that includes the vob subtile has been fixed.

 

5)      Network 

-          Support for deleting files on network folder has been added (*Netshare isn¡¯t supported)

-          Improved NFS speed (High bit rate movie will play better even with 10/100 connection )

¡¤         In case you have problem with 1G LAN, we recommend to use 10/100M mode.

(1G option may or may not work better than 10/100M mode depends on the network environment)

 

6)      UJukebox

-          External subtitle when playing ISO file is supported but the name of subtitle should be same as the ISO file

TViX can show two different subtitle in at the same time when selecting the external subtitle. 

-          Position of internal subtitle can be adjusted.

¡¤         How to : After pressing the subtitle key on the remote, while the ¡®subtitle mode¡¯ OSD is shown, press the up/down key on the remote

(for internal/external text subtitle, after pressing the subtitle key on the remote, you can  adjust the position and size of it as well)

 

7)      Etc

-          Improved UI : appearance of  some icons  have been enhanced.

-          Keeps separate BCS value according to output Hz (23.976, 24, 25, 29.97, 30, 50, 59.94 and 60Hz)

 

 - Known issues for Video related
    - Some TP/TS information may not correct.
    - When HD Audio pass-through is on, S/PDIF does not output.
    - When HD Audio pass-through is off with HD audio stream, the playback is not smooth.
        ¡Û When DTS audio setting is digital, HDMI audio is ON and HD audio passthrough is set to ON, then audio is not heard on the SPDIF output.
        ¡Û For the same setting, if HDMI audio is set to OFF, then audio is HEARD on the SPDIF output.
    - Some TP/TS files may cause the system rebooting.
    - Some WMV may not play correctly.
    - The digital output for AAC/WMA is disabled.
    - Does not support PCM audio track on MP4 now.
    - Some low sampling frequency on AVI and MKV may not sound on HDMI.
    - Some MKV with AAC may not sound.    

  - Known issues for Audio and pictures playing 
    - For MP3 files with low sampling frequency, the TVIX might crash while playing or trick play like FF or RW.
    
  - Known issues for PVR
    - After channel changed, you may not here audio in short time. This is the bug from the chip manufacturer. To solve this, you can press DTV key or Audio key on the remote.

  - Known issues for general issues.
    - If you play files without refreshing the file list after delete files through FTP or SAMBA server, the system will reboot.

    *** If you play files with HD audio tracks like Dolby TrueHD, , Dolby Digital Plus, DTS-HD MA or LPCM, you better turn on HD Audio pass through on the setup even though you don¡¯t have a receiver that supports decoding of these formats. Otherwise, you will hear strange noise with some repetitive popping noise. Currently, we don¡¯t support core decoding, if you don¡¯t have a HD audio decoder receiver, you need to select other then these HD audio tracks audio track for now.

This version of the firmware is for closed alpha testers and partners only.
Please do not distribute it publicly.
